Possible issues

# Open5gs

* Copy and make backup of each file before editing.
* Sometimes indentation problem in *yaml* file is not easily visible, in such case comparing difference between the original (backup) and edited file is helpful. *(using diff command)*
* In case no logs are registered in *mme.log*, deleting the *mme.log* file and creating new one is helpful. (one way to identify problem with *mme.log* file is checking status of *open5gs-mmed,* it keeps switching between active and activating)

# eNodeB

* Copy and make backup of each file before editing.
* Edit the correct *enb.conf* file, the correct file is located somewhere *../.config/srsran/enb.conf*. ***Locate*** command can be used to locate the directory of the same file.